**Site Visit Report**

|  |  |
| --- | --- |
| Date: | 12 February 2021 |
| Tender: | Tender for Plastering, Painting, Tile-Laying, the Manufacture, Supply, Delivery and Installation of Aluminium Apertures, Two Garage Doors, and a Spiral Staircase as part of ERDF Project ERDF.05.121 – Wildlife Rehabilitation Centre - ERDF.05.0121 – Tender 030 |
| Attendees: | As per attached signature sheet |
| Summary of Proceedings | Project Architect and representative of Project Management Service Provider gave a brief description of the nature of services expected under the tender document. The following questions were asked:Q1. Tender is generic re paint. Does it have to be Acrylic? Bidders should refer to the tender specs which focus on the performance of the paint, and not what type of paint it should be. The contractor will have to remove any existing finishes prior to applying any paint, and if necessary repair the surfaces.Q2. Does the floor have to be treated prior to the application of epoxy?The contractor will have to skim the ‘canals’ which cross the floor to a dept of circa six inches. Q3. With regards to the plastering of the ceiling, do the slabs (planki) have to be plastered over? The slabs (planki) themselves may not be plastered provided their surface is sufficiently smooth and ready to be painted over. Off course one would have to fill in the gaps. There will be areas where the ceiling is to be plastered over. Bidders should quote an average price. |

Project Manager

ERDF 05.121 – Wildlife Rehabilitation Centre